Return-Path: <bdu95398@strath.ac.uk>
Received: from lismore.cc.strath.ac.uk (lismore.cc.strath.ac.uk [130.159.248.18])
	by hugin.oden.se (8.8.5/8.8.5) with SMTP id CAA20531
	for <dlanor@oden.se>; Mon, 9 Jun 1997 02:41:52 +0200
Received: from lismore.cc.strath.ac.uk [130.159.96.148] 
	by lismore.cc.strath.ac.uk with smtp (Exim 1.61 #3)
	id 0wasWA-0002HN-00; Mon, 9 Jun 1997 01:41:06 +0100
To: <dlanor@oden.se>
Subject: laceScan
From: David Beaton <bdu95398@strath.ac.uk>
X-Mailer: Ant-Mail Version 0.7.9 (Atari) 
Message-Id: <E0wasWA-0002HN-00@lismore.cc.strath.ac.uk>
Date: Mon, 9 Jun 1997 01:41:06 +0100
X-UIDL: d5d909108e81129d95707139833df27a


I'm in the proccess of altering my  TOS 1.4 520ST FM (with 4Mb 
Marpet) to fit the lacescan circuit board.

I have two problems:

The first problem is that I don't know which ACIA chip is the
keyboard one.

The second problem is that on my computer the 5th pins on the
two ACIA chips are not connected as the instuction say they are.
Could the instructions mean pins 20 as these are joined together
on my computer?

Thank you in advance for any advice,

David Beaton.

.
