Received: from smtp.algonet.se (angel.algonet.se [194.213.74.112])
	by maskin.oden.se (8.8.7/8.8.7) with SMTP id GAA14521
	for <dlanor@oden.se>; Sat, 22 Nov 1997 06:02:42 +0100 (MET)
Received: (qmail 27549 invoked from network); 22 Nov 1997 05:04:41 -0000
Received: from du114-91.ppp.algonet.se (HELO algonet.se.news.algonet.se) (195.100.91.114)
  by angel.algonet.se with SMTP; 22 Nov 1997 05:04:41 -0000
From: "Martin Graiter" <magrait@algonet.se>
To: <dlanor@oden.se>
Subject: TOS-GAL
Date: Sat, 22 Nov 1997 06:08:15 +0100
Message-ID: <01bcf704$beb82400$725b64c3@algonet.se.news.algonet.se>
MIME-Version: 1.0
Content-Type: multipart/mixed;
	boundary="----=_NextPart_000_0099_01BCF70D.207C8C00"
X-Priority: 3
X-MSMail-Priority: Normal
X-Mailer: Microsoft Outlook Express 4.71.1712.3
X-MimeOLE: Produced By Microsoft MimeOLE V4.71.1712.3
X-UIDL: 6b79f433616b1b2c1f93b33fa3469d9d

Det här är ett multipart-meddelande i MIME-format.

------=_NextPart_000_0099_01BCF70D.207C8C00
Content-Type: text/plain;
	charset="iso-8859-1"
Content-Transfer-Encoding: 8bit

Hej igen,
Har hittat filen med TOS-adaptern, kan du göra ett försök?
Tror inte det är samma format som Maxon använder?

Martin






------=_NextPart_000_0099_01BCF70D.207C8C00
Content-Type: text/plain;
	name="Adapgal2.txt"
Content-Transfer-Encoding: quoted-printable
Content-Disposition: attachment;
	filename="Adapgal2.txt"

*IDENTIFICATION
Adressdecoder-GAL2 mit Umschaltm=94glichkeit zwishen altem und neuen TOS
30.07.1992 by WWS
erzeugt DTACK-Signal bei Speicherzugriffen auf $E00000 bis $E3FFFF
*X-NAMES
r_w, a18, a19, a20, a21, a22, a23, as, masse, ce_in, sel;
*Y-NAMES
dtack, ce_out, ce;
*LEVEL
HIGH;
LOW =3D as, ce_in, ce_out, ce;
*BOOLEAN-EQUATIONS
dtack =3D masse;
dtack.oe =3D a23 & a22 & a21 & /a20 & /a19 & /a18 & r_w & as;
ce_out=3Dce_in & sel;
ce_out.oe=3DVCC;
ce =3D a23 & a22 & a21 & /a20 & /a19 & /a18 & r_w & as & /sel
+ ce_in & /sel;
ce.oe =3DVCC;
*PLD
TYPE =3D GAL16V8_C7;
CHECKSUM =3D COMPUTE;
*PINS
r_w =3D 1, a18 =3D 3, a19 =3D4, a20 =3D5, a21 =3D6, a22 =3D7, a23 =3D8,
as =3D 9, masse =3D 11, dtack =3D 12, ce_in =3D 13, ce_out =3D 14,
sel =3D16,
ce =3D17;
*RUN-CONTROL
LISTING =3D SYMBOLTAB, NETTAB, EQUATIONS, PINOUT, FUSEPLOT;
PROGFORMAT =3D JEDEC;
*END
=20

------=_NextPart_000_0099_01BCF70D.207C8C00--


.
