Return-Path: <gooseman@on.ON-Luebeck.DE>
Received: from on.ON-Luebeck.DE (on.ON-Luebeck.DE [193.29.188.2])
          by hugin.oden.se (8.8.4/8.8.4) with ESMTP
	  id PAA12528 for <dlanor@oden.se>; Thu, 16 Jan 1997 15:49:40 +0100
Received: (from majordomo@localhost)
          by on.ON-Luebeck.DE (8.8.4/8.8.4)
	  id PAA25678 for stik-outgoing; Thu, 16 Jan 1997 15:11:16 +0100
Date: Thu, 16 Jan 1997 13:12:33 +0100 (MET)
From: Peter Rottengatter <perot@pallas.amp.uni-hannover.de>
To: STiK Development <stik@ON-Luebeck.DE>
Subject: STIK: More progress
Message-Id: <Pine.A32.3.91.970116130722.18572D-100000@pallas.amp.uni-hannover.de>
Mime-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII
Sender: stik@ON-Luebeck.DE
Precedence: bulk
Reply-To: stik@ON-Luebeck.DE
X-UIDL: b74d65887c1b7131a0c792d6700a4892



Another success : Have a traceroute working. When tracing the route to my 
university workstations I found that ICMP replies sent by AIX (Unix by 
IBM) do not completely comply with the RFC ;-) Anyway, I'll prepare 
another STiK V2.0 release soon with both ping and traceroute so that you 
can experiment with them too. I'll add a description on how to establish 
a modem connection without dialer. Actually the Dialer is the next I'll 
be busy with. It's just doing some modifications to the Dialer you've 
seen already, so I guess it won't take too much time.


Cheers  Peter

---------------------------------------------------------------------
   Peter Rottengatter             perot@pallas.amp.uni-hannover.de
---------------------------------------------------------------------

.
