Notes on PCB_Designer update 7-22-86

   -  handles 6 (6.3) by 4.5 inches (4.4 accessable 0.1 for border)

   -  can read all files of ST eurocard version (board files with board
      dimensions)

   -  prints layouts on EPSON FX100

   -  printout of layout in double speed (using only two instaed of four
      passes)

   -  Component plan will be printed out in one pass without reverse linefeed
      (was really hard work)

   -  boards and component plans smaller than 4.00 inches (width) can still be
      printed out on an EPSON FX80

   -  now without plotterdriver because the EPSON HI80 is now not able to
      handle either boards with maximum length or maximum width

New output drivers are currently being written, both for plotters and laser
printers.  Update notices will be send to all registered users, please
send in the warranty registration card to recieve the update notices.
