Computer:
TT030 with TOS 3.06, motherboard rev. H
internal & external 1.44 floppy drive
4MB ST RAM
16MB TT RAM
CPU modified to 48MHz with CaTTamaran, by Cybercube Research
(CaTT was professionally installed)

Graphics:

Cyrel, Sunrise M16-1280 graphics card, by Cybercube Research run at 
1280x1024x256 on an 18" SVGA ViewSonic Professional Series PS790
Desktop pattern through Ambiance by Cybercube Research

Peripherals:
 
1.44 external floppy drive
Syquest 135 EZ SCSI-2
Pioneer CD ROM, DRM-602X SCSI 6 CD changer 
*Atari SLM-605 Laser printer
HP Deskjet 660C printer
ZyXEL Elite 2864 V.34/FAX/Voice modem
Digital Series Hi-Fi stereo speakers

Important software:

HD Driver 7.61 for a hard drives running all read & write caches 
with this software. 
Geneva v 1.0 rel 006
NeoDesk 4 v 4 rel 005
NVDI 5 v 5.03
 

*  Note this may cause some unique DMA and ACSI problems with some code.
   One issue is the laser printer must be on if it is attached, or it will
   crash the booting process if it in not on during booting.

