March 12, 2005



IMPORTANT!

There are two versions of Just Musix 4:



standard.prg
------------------------------------------------------------
This is a reduced version of Just Musix 4 that replay
the music at 32kHz, and should work with a 16MHz 030-Falcon.

There's no moving effect or scroller here, only a timer 
clock and a menu selector. please read the file jm4.txt
history part for details about why this version is so simple.

There's a slight problem at the start on slower machines
as well; a slight colour flickering during colour fades.
It's a Falcon bug and the Graoumf routine kicks the VBL 
into the screen so the flickering becomes visible.



accelera.prg
------------------------------------------------------------
This is the real version of Just Musix 4 that replay the 
music at 49kHz, and includes a little graphical effect as
well as a scrolltext.

We have only been able to test the demo on CT2 and CT60,
other accelerators are unknown. Please be alarmed that
you might need to run the standard.prg on other accelerators!




------------->  CT60!!!  <-----------------------------------

                Due to the unsynced DSP-modreplayer, CT60
                users MUST disable CPU-caches before starting
                Just Musix 4, and that goes for both 
                versions of the demo. There's no way around
                this. We have run it on a standard 060/66
                without motherboard boost - it has behaved 
                fine. It is UNTESTED with other CT60
                configurations. Perhaps a 060/66+DSP boost
                can work with caches on? It's unknown.
 
 
 
 Thanks for reading.
 
 
 eof