    AFTERBURNER040 @ 20/40/80MHz
    Nemesis fitted and running with 20MHz bus
    Falcon 030 TOS 4.04
    AES v3.40
    GEMDOS v0.48
    MiNT not present
    Blitter not present
    NVDI 2.51 present
    Video Mode: 640*480*2
    FPU cookie value=$80000 (68040 internal)
    Run and Malloc from FastRAM
    Ref: F030 + FPU, 640*480*2

    GEM Dialog Box:             0.690    507%
    VDI Text:                   0.175   1942%
    VDI Text Effects:           0.365   2052%
    VDI Small Text:             0.225   1666%
    VDI Graphics:               0.920    948%
    GEM Window:                 0.485    288%
    Integer Division:           0.750    413%
    Float Math:                 0.080    425%
    RAM Access:                 0.180   1222%
    ROM Access:                 0.180   1166%
    Blitting:                   0.770    145%
    VDI Scroll:                 1.030    256%
    Justified Text:             0.835    390%
    VDI Enquire:                0.095   1663%
    New Dialogs:                0.800    556%

    Graphics:                            946%
    CPU:                                 806%
    Average:                             909%
Nemesis 5 / 6
|  | # 77