| #### Die Konfiguration ihres PoPs In der letzten Ausgabe der Revolution riefen wir die Leser mit Internet-Zugang auf, die Konfiguration für ihren PoP einzusenden, um die Anwender bei der Einrichtung und Konfiguration zu unterstützen. Steffen Reitinger hat uns freundlicherweise seine Konfiguration für den CSLIP-Zugang von T-Online überlassen. DIAL.SCR # #ACHTUNG! Alle Kommentare entfernt! # # noch eintragen an Stelle von A Anschlußkennung # M Mitbenutzerkennung # P Paßwort # Vorname & Nachname ersetzen # # RESIDENT = TRUE # PROTOCOL = 0 # VJHC = TRUE # LAN_PORT = FALSE # USERNAME = Vorname HOSTNAME = t-online.de FULLNAME = Vorname Nachname # CLIENT_IP = 0.0.0.0 # MTU = 576 # NAMESERVER = 130.75.1.32 NAMESERVER = 130.75.1.40 NAMESERVER = 194.25.2.129 NAMESERVER = 134.102.20.20 # SERIALPORT = Modem 1 # PHONE_NUMBER = 01910 # FEE_FILE = LOCAL.FEE # ISP_TIME = 60s, 0.05 ISP_SENT = 12K, 0.00 ISP_RECVD = 84K, 0.00 # DEF_ROUTE = TRUE # PTP_ROUTE = FALSE # EXEC_BATCH = FALSE # INIT = ATZ # PREFIX = ATDT # HANGUP = ,+++,ATH # CONNECT_WAIT = 60 REDIAL_DELAY = 20 # SUCCESS = CONNECT SUCCESS = CDWAIT FAILURE = BUSY FAILURE = NO CARRIER ABORT = NO DIALTONE # FIND_TIMEOUT = 60 # DIAL_SCRIPT # WAIT = 500 REPT = FIND = RESP = . # WAIT = 500 REPT = FIND = kennung: RESP = AAAAAAAAAAAAMMMMPPPPPPPP # WAIT = 1000 REPT = FIND = [?25h RESP = *53 # WAIT = 1000 REPT = FIND = ausgeschaltet RESP = *190144100 # WAIT = 1000 REPT = FIND = ER-Verb RESP = 19 # WAIT = 1000 REPT = FIND = STATUS OK RESP = LIN # WAIT = 500 REPT = FIND = RESP = OK # WAIT = 500 REPT = FIND = YOURIP RESP = $GET_IP Die Konfiguration Ihres PoPs - 1 / 1
|  | # 102