#### Technische Daten und Support für CENTurbo II Wie sie an den vorstehenden Benchmarks sicher ablesen können, bricht das CENTurbo II Board alle bisherigen Rekorde, es überholt auch den Afterburner in einigen Bereichen spielend. Wer den CENTEK-Falcon in Schaafheim "in Action" gesehen hat, wer da mitbekam, mit welcher Geschwindigkeit bekannte Software auf diesem Rechner gelaufen ist, wird sicher wissen von was hier die Rede ist. CENTurbo II ist das erste Beschleunigerboard, das einen Falcon auf reale 50 Mhz Takt bei vollständiger Systemstabilität bringt. Bei dieser Entwicklung wurden mehrere Wege eingeschlagen; Wege die u.a auch schon bei einigen anderen Entwicklungen versuchsweise ausprobiert wurden, aber nie zu diesen phänomenalen Resultaten führten. Modifikationen an der gesamten Hardware eröffnen hier eine ungeahnte Systemperformance. Ich unterliege hier der Versuchung, diesen Beschleuniger als den Hardwareknaller der letzten 24 Monate zu bezeichnen. Ein echtes Hammerteil - kaufen, Leute, kaufen! Nachfolgend finden Sie einige technische Daten und einige Worte zum Lieferumfang dieses Beschleunigers. a new CPU 68030 32-Bit at 50 MHz permanently! a SIMM 32-Bit standard socket offers 32-Bit EDO Fast-RAM (16 or 32 MB) acceded 7 times quicker than on original 16 MHz ST-Ram thanks to the 6..2.2.2 BURST accesses of the 030 (32 MB/s) at 50 MHz. a socket for a 32-Bit COPROCESSOR (68882-33) at 50 MHz. the DSP of the Falcon is clocked at 50 MHz. the BUS of the Falcon is clocked at 50 MHz (the CPU accesses at 50 MHz !). a 32-Bit Direct CPU BUS Slot, compatible extension of the Falcon BUS Slot will be available allowing you to use your 'old' cards (but not in the original case). Hardware documentation AVAILABLE for Hardware Designers ! on board 64 KB FLASH Eprom containing a new SET UP (NVRAM) and the BOOT of DOLMEN FALCON. DOLMEN FALCON. The new and ultra powered MULTITASKING Operating Sytem. DOLMEN FALCON is 100% ASM and TOS (AES & VDI) compatible ! a hardware switch enables you to come back to the 100% Falcon original mode. Wonderfully designed, the CENTurbo II fits in the original case within being embedded in the bus slot, needing only 12 wires soldering. CENTURBO II Falcon Speeder - 8 / 9
|  |  | # 102