| Two features are different with the final version of the CENTurbo II: the FPU is actually accessed by a 16-Bit DATA bus on the Falcon motherboard. It will be placed on the CT2 and accessed by a 32-Bit DATA bus... This increases the FPU performances of about 20%. the AES of DOLMEN is not the final version.
    RAM RATE measured with NEMBENCH (TITAN) and DAVEBENCH (CENTEK) :

    ORIGINAL FALCON            4,5 MB/s
    F030 + CT1 e2/e3 (ST-Ram)  7,5 MB/s
    F030 + CT2 Rev A FAST-Ram 31,7 MB/s
    F030 + AB40 FAST-Ram      34,5 MB/s

    400 % MANDELBROT FRACTAL COMPUTING with FRACTAL.PRG :

    Time in seconds :            CPU   FPU   DSP
    ORIGINAL FALCON              39.7 63.5   4.3
    F030 + CT1 25MHz ST-RAM      24.3 30.1   2.7
    F030 + CT2 50MHz FAST-Ram    10.0 18.1   1.9
    AB040                         7.2  5.0   2.6
Centurbo II - 13 / 42