Pin Freeze File:  version M.81d

95144XL100 XC95144XL-10-TQ100
a<0> S:PIN42
a<10> S:PIN10
a<11> S:PIN11
a<12> S:PIN12
a<13> S:PIN13
a<14> S:PIN14
a<15> S:PIN15
a<1> S:PIN50
a<2> S:PIN35
a<3> S:PIN36
a<4> S:PIN1
a<5> S:PIN3
a<6> S:PIN4
a<7> S:PIN6
a<8> S:PIN8
a<9> S:PIN9
activate_n_in S:PIN46
cartemu_enable_n S:PIN7
dualpokey_n S:PIN34
extsel_in S:PIN2
flash_we_n S:PIN19
irq_in S:PIN49
mpd_in S:PIN23
nc_adr<1> S:PIN71
nc_adr<2> S:PIN72
nc_adr<3> S:PIN74
nc_adr<4> S:PIN76
oldos_n S:PIN43
phi2 S:PIN22
phi2short S:PIN27
ramdisk_enable_n S:PIN24
reset_n_in S:PIN99
rw S:PIN33
refresh S:PIN73
d<0> S:PIN16
d<1> S:PIN17
d<2> S:PIN18
d<3> S:PIN20
d<4> S:PIN25
d<5> S:PIN28
d<6> S:PIN29
d<7> S:PIN30
ram0_ce S:PIN81
ram1_ce S:PIN96
ram_a<4> S:PIN92
ram_a<5> S:PIN93
ram_a<6> S:PIN94
ram_a<7> S:PIN95
ram_rom_a<12> S:PIN82
ram_rom_a<13> S:PIN85
ram_rom_a<14> S:PIN86
ram_rom_a<15> S:PIN87
ram_rom_a<16> S:PIN89
ram_rom_a<17> S:PIN90
ram_rom_a<18> S:PIN91
ram_rom_oe S:PIN78
ram_rom_we S:PIN77
rom0_ce S:PIN79
rom1_ce S:PIN97


;The remaining section of the .gyd file is for documentation purposes only.
;It shows where your internal equations were placed in the last successful fit.

PARTITION FB1_1 EXP14_ use_cartemu/cfg_enable use_cartemu/cfg_sram_bank_not0001/use_cartemu/cfg_sram_bank_not0001_D2 use_cartemu/cfg_mode<0>
		 $OpTx$FX_DC$510 use_cartemu/cfg_bank<5> use_cartemu/cfg_bank<4> use_cartemu/cfg_bank<3>
		 merged_out_dout<0> use_cartemu/cfg_bank<2> merged_out_dout<1> merged_out_dout<2>
		 use_cartemu/cfg_bank<1> use_cartemu/cfg_bank<0> merged_out_dout<3> dout_enable
		 EXP15_ use_cartemu/cfg_write_enable
PARTITION FB2_1 use_cartemu/N4/use_cartemu/N4_D2 use_cartemu/usdx_bank<4> use_cartemu/usdx_bank<3> use_cartemu/usdx_bank<2>
		 use_cartemu/usdx_bank<1> use_cartemu/cfg_sram_bank<4> use_cartemu/cfg_sram_bank<3> use_cartemu/cfg_sram_bank<2>
		 use_cartemu/cfg_sram_bank<1> use_cartemu/SFDecomp_100/use_cartemu/SFDecomp_100_D2 use_cartemu/usdx_ctl<1> use_cartemu/usdx_ctl<0>
		 use_cartemu/address_17_mux0003/use_cartemu/address_17_mux0003_D2 use_cartemu/address_16_mux0003/use_cartemu/address_16_mux0003_D2 use_cartemu/address_15_mux0003/use_cartemu/address_15_mux0003_D2 $OpTx$FX_DC$577
		 $OpTx$FX_DC$571 use_cartemu/do_access_mux0005/use_cartemu/do_access_mux0005_D2
PARTITION FB3_1 $OpTx$FX_DC$508 use_freezer/vector_a2 use_cartemu/address_19_and0000/use_cartemu/address_19_and0000_D2 use_cartemu/N97/use_cartemu/N97_D2
		 use_freezer/next_state_FSM_FFd3 merged_out_dout<4> use_freezer/next_state_FSM_FFd2 use_freezer/next_state_FSM_FFd1
		 merged_out_dout<5> use_cartemu/cfg_bank<6> merged_out_dout<6> merged_out_dout<7>
		 use_freezer/ram_bank_4 use_freezer/ram_bank_3 use_freezer/ram_bank_2 use_freezer/ram_bank_1
		 use_freezer/ram_bank_0 $OpTx$BIN_STEP$760
PARTITION FB4_1 $OpTx$FX_SC$591 ram_rom_a_15_OBUF $OpTx$FX_SC$586 $OpTx$FX_DC$521
		 ram_rom_a_16_OBUF ram_rom_a_17_OBUF $OpTx$FX_DC$499 ram_rom_a_18_OBUF
		 ram_a_4_OBUF use_freezer/N24/use_freezer/N24_D2 ram_a_5_OBUF ram_a_6_OBUF
		 freezer_mem_dout<5>/freezer_mem_dout<5>_D2 ram_a_7_OBUF ram1_ce_OBUF $OpTx$FX_DC$538
		 rom1_ce_OBUF merged_out_dout_or0000/merged_out_dout_or0000_D2
PARTITION FB5_1 use_freezer/next_state_cmp_eq0001/use_freezer/next_state_cmp_eq0001_D2 $OpTx$FX_DC$580 use_pia/pia_portb<4> use_pia/pia_portb<3>
		 use_pia/pia_portb<2> use_pia/pia_ddrb<7> use_pia/pia_ddrb<6> use_pia/pia_ddrb<5>
		 use_pia/pia_ddrb<4> use_pia/pia_ddrb<3> use_pia/pia_ddrb<2> use_cartemu/usdx_bank<5>
		 use_cartemu/usdx_bank<0> use_cartemu/oss_bank<1> use_cartemu/oss_bank<0> use_freezer/rom_bank_5
		 use_freezer/rom_bank_4 use_freezer/rom_bank_3
PARTITION FB6_5 EXP16_ ram_rom_we_OBUF N0/N0_TRST ram_rom_oe_OBUF
		 rom0_ce_OBUF use_cartemu/cart_disable_atari/use_cartemu/cart_disable_atari_D2 use_cartemu/N29/use_cartemu/N29_D2 ram0_ce_OBUF
		 $OpTx$FX_DC$601 ram_rom_a_12_OBUF ram_rom_a_13_OBUF use_cartemu/cctl_dout_and0000/use_cartemu/cctl_dout_and0000_D2
		 ram_rom_a_14_OBUF $OpTx$FX_DC$522
PARTITION FB7_1 use_freezer/state<2> use_freezer/state<1> use_freezer/state<0> reset_n_sync<3>
		 reset_n_sync<2> reset_n_sync<1> reset_n_sync<0> ramdisk_mem_adr<19>/ramdisk_mem_adr<19>_D2
		 powerup_n activate_n_sync<1> activate_n_sync<0> use_pia/pia_portb<7>
		 use_pia/pia_portb<6> use_pia/pia_portb<5> use_cartemu/cfg_sram_bank<5> use_cartemu/cfg_sram_bank<0>
		 $OpTx$FX_DC$608 $OpTx$FX_DC$540
PARTITION FB8_1 use_pia/pia_portb_0__or0000/use_pia/pia_portb_0__or0000_D2 use_pia/pia_ddrb_0__or0000/use_pia/pia_ddrb_0__or0000_D2 use_pia/pia_crb2 use_cartemu/cfg_usdx<1>
		 use_cartemu/cfg_usdx<0> use_cartemu/cfg_source_ram use_cartemu/cfg_mode<2> use_cartemu/cfg_mode<1>
		 use_cartemu/cfg_sram_enable use_cartemu/cfg_menu use_freezer/use_status_as_ram_address<0> use_freezer/rom_bank_2
		 use_freezer/rom_bank_1 use_freezer/rom_bank_0 use_cartemu/trig3_disable_atari $OpTx$INV$490
		 N0 use_cartemu/N50/use_cartemu/N50_D2

