### Compiler Options

Option | Value
--- | ---
Device(s) Specified | xc95144xl-10-TQ100
Optimization Method | DENSITY
Multi-Level Logic Optimization | ON
Ignore Timing Specifications | OFF
Default Register Power Up Value | LOW
Slew Rate | SLOW
Keep User Location Constraints | ON
What-You-See-Is-What-You-Get | OFF
Exhaustive Fitting | OFF
Keep Unused Inputs | ON
Power Mode | LOW
Ground on Unused IOs | ON
Global Clock Optimization | ON
Global Set/Reset Optimization | ON
Global Ouput Enable Optimization | ON
Set I/O Pin Termination | KEEPER
Input Limit (2-54) | 18
Pterm Limit (1-90) | 90