

               --- DSP 56000 Lod Disassembler ---



 usage: [-flags] file.lod [file.asm]

 flags: (-)p  you can see the operation in screen
        (-)i  the disassembler uses '<<' symbol ( MOVEP )
        (-)d  the disassembler uses the standard i/o labels
        (-)m  you can choose manual the disassembling mode
              when the disassembing is in the P memory!

 example: -pm echo.lod test.asm

 This program is share & postcardware ! ( For girls: Kissware !!! )
 If you can use this little program & find it useable
 please send 5 US dollar.

 Release date: 13 June 1993

     Gabriel Sebestyen      email: szoli@palma1.elte.hu
          Damjanich 23
         1071 BUDAPEST
	     HUNGARY

 p.s.: Hey somebody ! Please help me ! Send me a normal DSP assembler !
       I've got a very very shitty A56.TTP ! Thanx !!