| NEMESIS - VIDEO PERFORMANCE Falcon with Nemesis at 24/48MHz (24MHz System speed/48MHz DSP & FPU) all are non-interlaced resolutions, 16-bit (65,536 colours per screen) on a standard 14" VGA non-multisync! Expect far higher resolution modes with a half-decent multi-sync :-)
                     Bus    CPU    Video   Hz
    640x480          24     24     24      60
    720x528          24     24     24      50
Nemesis also accelerates the FPU and DSP to 48MHz. NEMESIS + AFTERBURNER040 - VIDEO PERFORMANCE Falcon with Afterburner040 and Nemesis - all are non-interlaced resolutions, 16-bit (65,536 colours per screen) on a standard 14" VGA.
                     Bus    CPU    Pipe   Video   Hz
    720x528          12.5   25     50     25      50
    640x480          12.5   25     50     25      60
    512x400          20     40     80     20      50
Note: Although the Afterburner CPU is being half-clocked in the highest resolutions, the actual performance is still much higher than a standard Falcon, and is completely switchable between the various specifications. Nähere Informationen können über die Homepage von Titan Design abgerufen werden. Ebenso können auch hier Bestellungen getätigt werden. Ein deutscher Händler, der den Nemesis vertreibt, ist mir bisher nicht bekannt. http://ourworld.compuserve.com/homepages/titanweb/ robscha@data.rhein-main.de Bilder, technische Daten und Benchmarks (c) Titan Design Ltd UK Nemesis - 6 / 6
|  | # 78