| #### AFTERBURNER/NEMESIS Benchmarks laut Hersteller
    AFTERBURNER040 @ 16.5/33/66MHz
    Standard Falcon

    Falcon 030 TOS 4.04
    AES v3.40
    GEMDOS v0.48
    MiNT not present
    Blitter not present
    NVDI 2.51 present
    Video Mode: 640*480*2
    FPU cookie value=$80000 (68040 internal)
    Run and Malloc from FastRAM
    Ref: F030 + FPU, 640*480*2
    GEM Dialog Box:             0.770    454%
    VDI Text:                   0.200   1700%
    VDI Text Effects:           0.410   1826%
    VDI Small Text:             0.250   1500%
    VDI Graphics:               1.045    835%
    GEM Window:                 0.535    261%
    Integer Division:           0.910    340%
    Float Math:                 0.095    357%
    RAM Access:                 0.215   1023%
    ROM Access:                 0.220    954%
    Blitting:                   0.875    128%
    VDI Scroll:                 1.140    231%
    Justified Text:             0.920    354%
    VDI Enquire:                0.110   1436%
    New Dialogs:                0.905    491%

    Graphics:                            837%
    CPU:                                 668%
    Average:                             792%
Nemesis - 4 / 6
|  | # 76