<?xml version='1.0' encoding='utf-8' ?>
<!DOCTYPE ibis [
<!ELEMENT ibis (part, pin+)>
<!ELEMENT part EMPTY>
<!ELEMENT pin EMPTY>
<!ATTLIST part
  arch   CDATA #REQUIRED
  device CDATA #REQUIRED
  spg    CDATA #REQUIRED
  pkg    CDATA #REQUIRED>
<!ATTLIST pin
  nm     CDATA #REQUIRED
  no     CDATA #REQUIRED
  iostd  (TTL|LVTTL|LVCMOS2|NA) "NA"
  sr     (SLOW|FAST|slow|fast) "SLOW"
  dir    (BIDIR|bidir|INPUT|input|OUTPUT|output) "BIDIR">
]>
<ibis><part arch="xc9500xl" device="XC95144XL" pkg="TQ100" spg="-10"/><pin dir="input" nm="a&lt;14&gt;" no="14"/><pin dir="input" nm="ramdisk_enable_n" no="24"/><pin dir="input" nm="a&lt;15&gt;" no="15"/><pin dir="input" nm="rw" no="33"/><pin dir="input" nm="a&lt;11&gt;" no="11"/><pin dir="input" nm="a&lt;9&gt;" no="9"/><pin dir="input" nm="a&lt;8&gt;" no="8"/><pin dir="input" nm="a&lt;10&gt;" no="10"/><pin dir="input" nm="a&lt;6&gt;" no="4"/><pin dir="input" nm="a&lt;5&gt;" no="3"/><pin dir="input" nm="a&lt;7&gt;" no="6"/><pin dir="input" nm="a&lt;3&gt;" no="36"/><pin dir="input" nm="a&lt;2&gt;" no="35"/><pin dir="input" nm="a&lt;1&gt;" no="50"/><pin dir="input" nm="a&lt;0&gt;" no="42"/><pin dir="input" nm="a&lt;4&gt;" no="1"/><pin dir="input" nm="phi2short" no="27"/><pin dir="input" nm="cartemu_enable_n" no="7"/><pin dir="input" nm="phi2" no="22"/><pin dir="input" nm="a&lt;13&gt;" no="13"/><pin dir="input" nm="a&lt;12&gt;" no="12"/><pin dir="input" nm="flash_we_n" no="19"/><pin dir="input" nm="oldos_n" no="43"/><pin dir="input" nm="dualpokey_n" no="34"/><pin dir="input" nm="activate_n_in" no="46"/><pin dir="input" nm="reset_n_in" no="99"/><pin dir="input" nm="extsel_in" no="2"/><pin dir="input" nm="irq_in" no="49"/><pin dir="input" nm="mpd_in" no="23"/><pin dir="input" nm="nc_adr&lt;1&gt;" no="71"/><pin dir="input" nm="nc_adr&lt;2&gt;" no="72"/><pin dir="input" nm="nc_adr&lt;3&gt;" no="74"/><pin dir="input" nm="nc_adr&lt;4&gt;" no="76"/><pin dir="output" nm="ram0_ce" no="81" sr="slow"/><pin dir="output" nm="ram1_ce" no="96" sr="slow"/><pin dir="output" nm="ram_a&lt;4&gt;" no="92" sr="slow"/><pin dir="output" nm="ram_a&lt;5&gt;" no="93" sr="slow"/><pin dir="output" nm="ram_a&lt;6&gt;" no="94" sr="slow"/><pin dir="output" nm="ram_a&lt;7&gt;" no="95" sr="slow"/><pin dir="output" nm="ram_rom_a&lt;12&gt;" no="82" sr="slow"/><pin dir="output" nm="ram_rom_a&lt;13&gt;" no="85" sr="slow"/><pin dir="output" nm="ram_rom_a&lt;14&gt;" no="86" sr="slow"/><pin dir="output" nm="ram_rom_a&lt;15&gt;" no="87" sr="slow"/><pin dir="output" nm="ram_rom_a&lt;16&gt;" no="89" sr="slow"/><pin dir="output" nm="ram_rom_a&lt;17&gt;" no="90" sr="slow"/><pin dir="output" nm="ram_rom_a&lt;18&gt;" no="91" sr="slow"/><pin dir="output" nm="ram_rom_oe" no="78" sr="slow"/><pin dir="output" nm="ram_rom_we" no="77" sr="slow"/><pin dir="output" nm="rom0_ce" no="79" sr="slow"/><pin dir="output" nm="rom1_ce" no="97" sr="slow"/><pin dir="output" nm="refresh" no="73" sr="slow"/><pin dir="bidir" nm="d&lt;0&gt;" no="16" sr="slow"/><pin dir="bidir" nm="d&lt;5&gt;" no="28" sr="slow"/><pin dir="bidir" nm="d&lt;1&gt;" no="17" sr="slow"/><pin dir="bidir" nm="d&lt;2&gt;" no="18" sr="slow"/><pin dir="bidir" nm="d&lt;3&gt;" no="20" sr="slow"/><pin dir="bidir" nm="d&lt;4&gt;" no="25" sr="slow"/><pin dir="bidir" nm="d&lt;6&gt;" no="29" sr="slow"/><pin dir="bidir" nm="d&lt;7&gt;" no="30" sr="slow"/></ibis>
